# HAZARD MARKING COLOUR APPLICATION GUIDELINES

| **APPLICATION** | **EXAMPLES** | **AS 2700 PAINT** |
| --- | --- | --- |
| Places where caution needs to be exercised (Yellow) | * Machine guards * Stairs (nosing – top and front - of top and bottom step) * Flammable liquid cabinets * Concrete lane separators and delineators on narrow ramps * Pillars, posts or columns exposed to traffic * Edges of temporary or movable ramps * Radiation hazards * Speed humps (Striped 150 mm wide) * Fixed ladders and cages (as needed) * Handrails (as needed) | Y15 (Sunflower) |
| Places where caution needs to be exercised (Yellow / Black stripes - min 75 mm wide @ 45o ) | * Projections * Overhead fixtures that project into operating space * Floor footprint of overhead hazards such as crane parking areas etc. * Low head room * Drop into pit or void * Change in height * Bollards and corner edging * Low pulley blocks and crane hooks * Covering and guards for guy wires * Corners of rotating machinery such as excavators and cranes * Swing room for outside opening doors | Y15 (Sunflower/ Black) |
| Floor marking for walkways (Yellow stripes - 75 mm wide) | * Aisles and walkways in workshops and warehouses | Y15 (Sunflower) |
| Floor marking for laydown and storage (Light Grey stripes - 75 mm wide) | * Workshops and warehouses | N35 (light grey) |
| Floor marking for work areas (Bright Blue stripes - 75 mm wide) | * Workshops and warehouses * Areas requiring use of PPE | B23 (Bright blue) |
| Keep clear areas for outward opening doors including exits (Yellow floor markings – 150 mm wide) | * Workshops and warehouses | Y15 (Sunflower) |
| Keep clear areas for FIRE equipment exclusively (Red floor markings – 150 mm wide) | * Workshops and warehouses | R13 (Signal red) |
| Keep clear areas, safety equipment, eye wash-stands (Green floor markings – 150 mm wide) | * Workshops and warehouses | G21 (Jade) |
| Fire equipment (wall marking - Red/white stripes - 75 mm wide @ 45o) | * Workshops and warehouses | R13 (Signal Red)/ White |
| Safety equipment (wall markings - Green/white stripes - 75 mm wide @ 45o) | * Workshops and warehouses | G21 (Jade)/White |

## MACHINERY AND EQUIPMENT

|  |  |  |  |
| --- | --- | --- | --- |
|  | APPLICATION | EXAMPLES | AS 2700 PAINT |
| Machinery pinch points (Red/white stripes - 75 mm wide @ 45o) | | * Mobile equipment articulation areas * Rear dump front wheel wells * Machinery pinch points | R13 (Signal Red)/ White |
| Machinery controls – shutdown and stop controls (red) | | * Stop buttons and emergency stop controls. * Stop buttons for electrical switches used for normal and emergency stopping of machinery. * Emergency stop bars on hazardous machines. * Emergency stop controls of any description. | R13 (Signal Red) |
| Machinery controls – start controls (Green) | | On buttons and controls | G21 (Jade) |