# HAZARD MARKING COLOUR APPLICATION GUIDELINES

| **APPLICATION** | **EXAMPLES** | **AS 2700 PAINT** |
| --- | --- | --- |
| Places where caution needs to be exercised (Yellow) | * Machine guards
* Stairs (nosing – top and front - of top and bottom step)
* Flammable liquid cabinets
* Concrete lane separators and delineators on narrow ramps
* Pillars, posts or columns exposed to traffic
* Edges of temporary or movable ramps
* Radiation hazards
* Speed humps (Striped 150 mm wide)
* Fixed ladders and cages (as needed)
* Handrails (as needed)
 | Y15 (Sunflower) |
| Places where caution needs to be exercised (Yellow / Black stripes - min 75 mm wide @ 45o ) | * Projections
* Overhead fixtures that project into operating space
* Floor footprint of overhead hazards such as crane parking areas etc.
* Low head room
* Drop into pit or void
* Change in height
* Bollards and corner edging
* Low pulley blocks and crane hooks
* Covering and guards for guy wires
* Corners of rotating machinery such as excavators and cranes
* Swing room for outside opening doors
 | Y15 (Sunflower/ Black) |
| Floor marking for walkways (Yellow stripes - 75 mm wide) | * Aisles and walkways in workshops and warehouses
 | Y15 (Sunflower) |
| Floor marking for laydown and storage (Light Grey stripes - 75 mm wide) | * Workshops and warehouses
 | N35 (light grey) |
| Floor marking for work areas (Bright Blue stripes - 75 mm wide) | * Workshops and warehouses
* Areas requiring use of PPE
 | B23 (Bright blue) |
| Keep clear areas for outward opening doors including exits (Yellow floor markings – 150 mm wide) | * Workshops and warehouses
 | Y15 (Sunflower) |
| Keep clear areas for FIRE equipment exclusively (Red floor markings – 150 mm wide) | * Workshops and warehouses
 | R13 (Signal red) |
| Keep clear areas, safety equipment, eye wash-stands (Green floor markings – 150 mm wide) | * Workshops and warehouses
 | G21 (Jade) |
| Fire equipment (wall marking - Red/white stripes - 75 mm wide @ 45o) | * Workshops and warehouses
 | R13 (Signal Red)/ White |
| Safety equipment (wall markings - Green/white stripes - 75 mm wide @ 45o) | * Workshops and warehouses
 | G21 (Jade)/White |

## MACHINERY AND EQUIPMENT

|  |  |  |  |
| --- | --- | --- | --- |
|  | APPLICATION | EXAMPLES | AS 2700 PAINT |
| Machinery pinch points (Red/white stripes - 75 mm wide @ 45o) | * Mobile equipment articulation areas
* Rear dump front wheel wells
* Machinery pinch points
 | R13 (Signal Red)/ White |
| Machinery controls – shutdown and stop controls (red) | * Stop buttons and emergency stop controls.
* Stop buttons for electrical switches used for normal and emergency stopping of machinery.
* Emergency stop bars on hazardous machines.
* Emergency stop controls of any description.
 | R13 (Signal Red) |
| Machinery controls – start controls (Green) | On buttons and controls | G21 (Jade) |